For Some Models (Driver's seat) SRS components are located in this area. Review the SRS component locations LHD, SRS component locations RHD and the precautions and procedures before performing repairs or service. NOTE:

- When prying components, use the handy remover set or equivalent.
- Take care not to bend the cable.
- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.

1. Remove these items:
   - Lumbar support knob
   - Back panel

1. Release the hook strips on the inside of the seat-back.

1. Remove the screws securing the lumbar support actuator (A).