1. To raise the rear portion of the engine, support the rear engine mount bracket with the jack stand (A) as shown in the following illustration.

1. Remove the loosened mounting bolt that holds the rear engine mount bracket, and remove the rear engine mount rubber. Then, pull up the rear engine mount rubber removed from its original position not to interfere with the removal of the steering gearbox.