For front seat belt retractor with seat belt tensioner, review the SRS component locations and the precautions and procedures before performing repairs or service. Retractor

1. Before installing the retractor, check that the seat belt can be pulled out freely.

1. Make sure that the seat belt does not lock when the retractor (A) is leaned slowly up to 15 ° from the mounted position. Do not attempt to disassemble the retractor.

Front

1. Make sure that the seat belt locks when the retractor is leaned over 40 ° from the mounted position. Do not attempt to disassemble the retractor.

Rear/Rear Center

1. Lean the retractor over 40 °, and make sure that the seat belt does not lock when pulled out over about 1,100 mm (43.3 in.). Do not attempt to disassemble the retractor.

1. Replace the seat belt with a new assembly if there is any abnormality. Do not disassemble any part of the seat belt for any reason.

Front
Rear/Rear center