Starter Reassembly

1. Pry back each brush spring with a screwdriver, then position the brush about halfway out of its holder, and release the spring to hold it there.
   NOTE: To seat the new brushes, slip a strip of #500 or #600 sandpaper, with the grit side out, between the commutator and each brush, and smoothly rotate the armature. The contact surface of the brushes will be sanded to the same contour as the commutator.