1. Attach the hanger plate (A) to the stud nut (B) on the ERG passage with 8 x 1.25−16 mm bolt (C). Use only the 8 x 1.25 mm and 16 mm in length of the threads bolt. If you use other than 16 mm threads-length bolt, it may damage the engine cylinder head.

1. Attach the hanger plate (D) to the threaded hole in the back of the cylinder head. Attach the hoist to the hanger plates, and lift and support the engine.Do not attach the hoist to the engine directly, always use the hanger plates.