1. Warm up the engine.

1. Remove the maintenance lid (A).

1. Remove the drain bolt (B), and drain the engine oil.

1. Reinstall the drain bolt with a new washer (C).

1. Refill with the recommended oil.

   Capacity
   At Oil Change:
   4.0 L (4.2 US qt, 3.5 Imp qt)
   At Oil Change including Filter:
   4.2 L (4.4 US qt, 3.7 Imp qt)
   After Engine Overhaul:
   5.3 L (5.6 US qt, 4.7 Imp qt)

1. Run the engine for more than 3 minutes, then check for oil leakage.