1. Measure voltage between fuel pressure control valve 2P connector terminal No. 1 and body ground.

Is there battery voltage?

YES | - | Repair short to power in the wire between in the wire between the fuel pressure control valve and ECM connector No. 1 terminal No. 79, then go to Step 11 .
NO | - | Go to Step 15 .

1. Replace the fuel supply pump assembly.

1. Reconnect all connectors.

1. Turn the ignition switch ON (II).

1. Reset the ECM with the HDS.

1. Check for Temporary DTCs or DTCs with the HDS.

Are any Temporary DTCs or DTCs indicated?

YES | - | If DTC P1057 is indicated, check for poor connections or loose terminals at the fuel pressure control valve and the ECM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | Troubleshooting is complete.■

1. Update the ECM if it does not have the latest software, or substitute a known-good ECM.

1. Check for Temporary DTCs or DTCs with the HDS.

Are any Temporary DTCs or DTCs indicated?

YES | - | If DTC P1057 is indicated, check for poor connections or loose terminals at the fuel pressure control valve and the ECM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | If the ECM was updated, troubleshooting is complete. If the ECM was substituted, replace the original ECM. ■