Installation

1. Install the new SRS unit (A) with Torx bolts (B), then connect the connectors (C) to the SRS unit; push them into position until they click.
   NOTE: Be sure the SRS unit is sitting squarely against it's bracket before torquing the Torx bolt.

1. Reconnect both seat belt tensioner connectors.

1. Reconnect the battery negative cable.

1. After installing the SRS unit, confirm proper system operation: Turn the ignition switch ON (II); the SRS indicator should come on for about 6 seconds and then go off.

1. Install all removed parts.