How to Clear DTCs NOTE: You cannot clear the DTCs manually.

1. With the ignition switch OFF, connect the HDS to the 16P data link connector (DLC) (A) under the driver's side of the dashboard.

1. Turn the ignition switch ON (II), and clear the DTC(s) by following the screen prompts on the HDS.
   NOTE: See the HDS Help menu for specific instructions.

1. Do the VSA sensor neutral position memorization.