1. Install the trim in the reverse order of removal, and note these items:
   - Replace any damaged clips with a new one.
   - Do not reuse the rear pillar cap; always replace it.
   - If the side curtain airbag has deployed, replace the rear pillar trim with new one.
   - To prevent the side curtain airbags from deploying improperly and possibly causing injury, inspect removed pieces and replace them if they have any of these types of damage.

   - | Any cracks, deformations, or stress-whitenings in the rear pillar trim (A)
   - | Any cracks, or stress-whitenings in the grommet and clip seating surfaces (B)
   - | Bent or broken grommet (C)

   - Replace any damaged parts with new ones.
   - Make sure the top of the trim overlaps with the headliner correctly.
   - Push the clips into place securely.