NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.
- Use the handy remover set, or equivalent when prying components.

1. Remove the seat cushion.

1. Remove the screws (A) and the dampers (B), pry the clips (C) with a handy remover, then remove the seat cushion base board (D). The right seat cushion is shown; the left seat cushion is similar.