1. Install the A/T clutch pressure control solenoid valve A connector and 2nd clutch transmission fluid pressure switch connector (B), and install the harness clamps (C) on the harness clamp brackets (D).

1. Refill the transmission with ATF.

1. Install the battery base.

1. Install the air cleaner housing and intake air duct.

1. Install the battery tray, battery, and battery cover, then secure the battery with its hold-down bracket.

1. Connect the battery terminals.

1. Set the parking brake. Start the engine, and shift the transmission through all gears three times.

1. Check the shift lever operation, A/T gear position indicator operation, and shift cable adjustment.

1. Check and adjust the front wheel alignment.

1. Install the splash shield.

1. Turn off the engine, and check the ATF level.

1. Do the power window control unit reset procedure.

1. Do the road test.

1. Enter the anti-theft code for the radio (and navigation system), then enter the radio station presets, and set the clock.