1. Install the intake air duct (A), then connect the intake air temperature (IAT) sensor connector (B), and install the vacuum hose (C) and breather pipe (D).

1. After installation, check that all tubes, hoses, and connectors are installed correctly.

1. Inspect for fuel leaks. Turn the ignition switch to ON (II) (do not operate the starter) so that the fuel pump runs for about 2 seconds and pressurizes the fuel line. Repeat this operation two or three times, then check for fuel leakage at any point in the fuel line.

1. Refill the radiator with engine coolant, and bleed air from the cooling system with the heater valve open.

1. Reset the power window control unit.

1. Inspect the idle speed.

1. Inspect the ignition timing.

1. Set the clock.