Camera for LKAS (Control unit integrated type)
The low power consumption type 1/4 inch. C. MOS * image pickup device camera is mounted on the roof rail above the room mirror with a built-in control unit. The lens is installed on the position which shifts 46 mm (1.81 inch.) from the center of the vehicle to the driver's side. The camera is constructed of a camera part (filter, lens, and image pickup device) and an image process part (image process circuit and CPU).
* C. MOS (Complementary Metal Oxide Semiconductor): Electrical charge storage in each pixel is converted to voltage and then amplified for the output.
The adaptive cruise control (ACC) system automatically controls the vehicle speed, within the set speed, to maintain a safe distance between the vehicle ahead.