1. Remove the hub bearing unit (A).

1. Install the hub bearing unit in the reverse order of removal, and note these items:
   - Tighten all mounting hardware to the specified torque values.
   - Use a new spindle nut on reassembly.
   - Wash the spline thoroughly in high flash point solvent before reassembly.
   - Before installing the spindle nut, apply a small amount of engine oil to the seating surface of the nut. After tightening, use a drift to stake the spindle nut shoulder against the driveshaft.
   - Before installing the brake disc/drum, clean the mating surfaces of the hub bearing unit and the brake disc/drum.
   - Before installing the wheel, clean the mating surfaces of the brake disc/drum and the inside of the wheel.
   - Check the wheel alignment, and adjust it if necessary.