1. Check for continuity between LKAS control unit 26P connector terminal No. 7 and LKAS camera 10P connector terminal No. 6.

Is there continuity?

YES | - | Check for loose terminals in the LKAS camera and LKAS control unit connectors, and repair if necessary. If no poor connections are found, replace the LKAS camera. ■
NO | - | Repair an open in the wire between LKAS camera and LKAS control unit.■