1. Install the buckle in the reverse order of removal, and note these items:
   - Assemble the washers and bushing on the center anchor bolt as shown.
   - Tighten the bolt by hand first, then tighten to specification with a torque wrench.
   - Reconnect the negative cable to the battery.
   - Perform the power window control unit reset procedure.
   - Reset the clock.

Center anchor bolt construction