Maintenance Schedule for Severe Conditions - Australia and New Zealand Models
140,000km(7year)

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35 °C (95 °F) conditions.
- Extensive idling, or long periods of stop-and-go-driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the customer's vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule.
Service at the indicated distance or time whichever comes first

| Replace air cleaner element

Use normal schedule except in dusty conditions

| Replace automatic transmission fluid

Use Honda ATF-Z1

| Check lights alignment

Check the position of the headlights

| Test drive

Check for road stability, noise, vibrations, and dashboard operation

Visually inspect the following items:

|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks
|  | Check tightness of screws, nuts, and joints. If necessary, retighten

| Brake hoses and lines (including ABS)

Check the master cylinder, proportioning control valve, and ABS modulator and leakage

| All fluid levels and condition of fluids

Check levels and check for leaks. If necessary, add engine coolant , MTF, ATF, brake fluid, windshield fluid, and battery fluid

| Exhaust system

Check the exhaust pipe and muffler for damage, leaks, and tightness

| Fuel lines and connections

Check fuel lines for loose connections, cracks, and deterioration. Retighten loose connections and replace any damaged parts

Every 5,000 km (3,125 miles) or 6 months

| Replace engine oil

Every 10,000 km (6,250 miles) or 6 months

| Replace engine oil filter

| Inspect front and rear brakes

|  | Check the brake pad and disc thickness. Check for damage or cracks front pad , front disc , rear pad , rear disc
|  | Check the calipers for damage, leaks, and tightness

Visually inspect the following items:

| Tie-rod ends, steering gearbox, and boots

Check rack grease and steering linkage. Check the boot for damage and leaking grease

| Suspension components

|  | Check the bolts for tightness
|  | Check all dust cover for deterioration and damage

| Driveshaft boots

|  | Check the boot and boot band for cracks
|  | Check rack grease

At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years

| Replace engine coolant

Use genuine Honda All Season Antifreeze/Coolant Type 2

Every 3 years

| Replace brake fluid

|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid
|  | Check that brake fluid level is between upper and lower marks on the reservoir

Every 30,000 km (18,750 miles) or 1 year

| Replace dust and pollen filter

Every 10,000 km (6,250 miles)

| Rotate tyres

Check tyre inflation and condition at least once per month