Trunk Latch Switch Test

1. Open the trunk lid.

1. Disconnect the 3P connector (A) from the trunk lid latch (B).

1. Check for continuity between the No. 2 and No. 3 terminals.
   - There should be continuity with the trunk lid latch unlatched (trunk open).
   - There should be no continuity with the trunk lid latch latched (trunk closed).

1. If the continuity is not as specified, replace the trunk lid latch switch.