Inspection (KQ Model)

1. Raise the front of the vehicle, and support it with safety stands in the proper locations.

1. Remove the front wheels.

1. Remove the brake pads.

1. Check the thickness of the brake pads (A). Do not include the thickness of the brake pad backing plate (B).

   Brake pad thickness:
   | Standard: | 10.5−11.5 mm (0.41−0.45 in.)
   | Service limit: | 1.6 mm (0.06 in.)

1. If the brake pad thickness is less than the service limit, replace all the pads as a set.