Engine Mount Replacement - Side

1. Support the engine with a jack and wood block under the oil pan.

1. Remove the ground cable (A), then remove the upper torque rod (B).

1. Remove the side engine mount bracket.

1. Remove the side engine mount.

1. Install the new side engine mount.

1. Install the side engine mount bracket (A), then loosely tighten the new bolts/nut (B), and loosely tighten the bolt (C).

1. Remove the air cleaner housing.

1. Loosen the transmission upper mount bracket bolt (A) and transmission upper mount bolt/nuts (B).

1. Remove a jack.

1. Tighten the side engine mount mounting bolts/nut in the numbered sequence shown.

1. Tighten the transmission upper mount/bracket mounting bolts/nuts in the numbered sequence shown.

1. Install the upper torque rod (A), then tighten the new bolts in the numbered sequence shown.

1. Install the ground cable (B).

1. Install the air cleaner housing.