1. Be careful not to damage the pressure plate (A). Tighten (180 degrees apart) the pressure plate mounting bolts (B) in a star pattern in several steps.

   Pressure Plate Mounting Bolt Torque:
   25 N·m (2.6 kgf·m, 19 lbf·ft)

1. Turn the center screw on the pressure plate compressor counterclockwise by hand to release the pressure, then remove the special tools.

1. Make sure the diaphragm spring fingers are all the same height.