NOTE:

- Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid gets on the paint, wash it off immediately with water.
- To prevent dripping brake fluid, cover disconnected hose joints with rags or shop towels.
- Do not twist the brake hose and line when removed.

1. Drain the brake fluid.

1. Disconnect the 3P connector (BLU) (A) from the right front pressure sensor (B).

1. Disconnect the 3P connector (GRY) (C) from the left front pressure sensor (D).

1. Remove the brake lines (E) from the 4-way joint (F).

1. Remove the brake 4-way joint.