Low Fuel Indicator Test

1. Do the gauge drive circuit check.
   - If the low fuel indicator flashes, go to Step 2 .
   - If the low fuel indicator does not flush, replace the gauge control module assembly.

1. Perform the multiplex integrated control system troubleshooting test mode A.
   - If any DTCs are indicated, do the indicated DTC's troubleshooting.
   - If no DTC's are indicated, go to Step 3 .

1. Perform fuel gauge sending unit test.