1. Open the driver's door, and remove the caps (A), then remove the bolts (B, C, D), and clips (E) and lift up on the dashboard (F)/steering hanger beam to release it from the guide pins (G, H).
   NOTE: Before removing the dashboard/steering hanger beam, make sure all the harnesses have been disconnected.

1. Carefully remove the dashboard/steering hanger beam through the front door opening.
   NOTE: Lay the dashboard/steering hanger beam on its front or back. Do not lay it on the lower console opening or you may damage it.