DTC 34-8x (34-80 to 34-89, 34-8A to 34-8F): Short to Power in Right Side Curtain Airbag Inflator Special Tools Required SRS inflator simulator 07SAZ-TB4011A
SRS simulator lead E
07XAZ-S1A0200

1. Erase the DTC memory.

1. Turn the ignition switch ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off.

Does the SRS indicator stay on and is DTC 34-8x indicated?

YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, go to the DTC troubleshooting index for troubleshooting details.

1. Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes.

1. Disconnect the right side curtain airbag 2P connector from the side curtain airbag subharness (A).

1. Connect the SRS inflator simulator (2 Ω connector) and simulator lead E to the side curtain airbag subharness.

1. Reconnect the battery negative cable.

1. Erase the DTC memory.

1. Read the DTC.

Is DTC 34-8x indicated?

YES | - | Go to Step 9 .
NO | - | Short to power in the right side curtain airbag inflator; replace the right side curtain airbag. ■

1. Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes.