Clutch - 3/4

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Clutch - 3/4 | 1st and 3rd clutch end-plate thickness (K20Z2 engine) | Mark 1 | 2.3 mm (0.090 in.) | When discolored
Mark 2 | 2.4 mm (0.094 in.) | When discolored
Mark 3 | 2.5 mm (0.098 in.) | When discolored
Mark 4 | 2.6 mm (0.102 in.) | When discolored
Mark 5 | 2.7 mm (0.106 in.) | When discolored
Mark 6 | 2.8 mm (0.110 in.) | When discolored
Mark 7 | 2.9 mm (0.114 in.) | When discolored
Mark 8 | 3.0 mm (0.118 in.) | When discolored
Mark 9 | 3.1 mm (0.122 in.) | When discolored
Mark 10 | 3.2 mm (0.126 in.) | When discolored
Mark 11 | 3.3 mm (0.130 in.) | When discolored
Mark 12 | 3.4 mm (0.134 in.) | When discolored
2nd clutch end-plate thickness (K20Z2 engine) | Mark 1 | 2.6 mm (0.102 in.) | When discolored
Mark 2 | 2.7 mm (0.106 in.) | When discolored
Mark 3 | 2.8 mm (0.110 in.) | When discolored
Mark 4 | 2.9 mm (0.114 in.) | When discolored
Mark 5 | 3.0 mm (0.118 in.) | When discolored
Mark 6 | 3.1 mm (0.122 in.) | When discolored
Mark 7 | 3.2 mm (0.126 in.) | When discolored
Mark 8 | 3.3 mm (0.130 in.) | When discolored
Mark 9 | 3.4 mm (0.134 in.) | When discolored
4th and 5th clutch end-plate thickness (K20Z2 engine) | Mark 1 | 3.0 mm (0.118 in.) | When discolored
Mark 2 | 3.1 mm (0.122 in.) | When discolored
Mark 3 | 3.2 mm (0.126 in.) | When discolored
Mark 4 | 3.3 mm (0.130 in.) | When discolored
Mark 5 | 3.4 mm (0.134 in.) | When discolored
Mark 6 | 3.5 mm (0.138 in.) | When discolored
Mark 7 | 3.6 mm (0.142 in.) | When discolored
Mark 8 | 3.7 mm (0.146 in.) | When discolored
Mark 9 | 3.8 mm (0.150 in.) | When discolored