DTC 51: Motor Lock DTC 52: Motor Stuck OFF

1. Check the No. 17 (30 A) fuse in the under-hood fuse/relay box.

Is the fuse OK?

YES | - | Reinstall the fuse, and go to Step 2 .
NO | - | Replace the fuse, and recheck.■

1. Disconnect the VSA control unit 47P connector.

1. Measure the voltage between the VSA control unit 47P connector terminal No. 1 and body ground.

Is there battery voltage?

YES | - | Go to Step 4 .
NO | - | Repair open in the wire between the No. 17 (30 A) fuse and the VSA modulator-control unit.■