1. Remove the tailgate lower trim panel (A).

   -1. | Pry up on the lid (B), remove the self-tapping ET screw (C) using a T25 Torx bit, then remove the tailgate pull pocket (D). If equipped, disconnect the power tailgate close switch connector (E).
   -2. | Release the clips (F).
   -3. | Pull out the trim panel to detach the clips (G, H).

1. Install the trim in the reverse order of removal, and note these items:
   - Replace any damaged clips.
   - If the threads on a pull pocket screw are worn out, use an oversized self-tapping ET screw, P/N90137-S1A-E01, made specifically for this application.
   - If equipped, make sure the power tailgate close switch connector is plugged in properly, and check the power tailgate operation.