How to Troubleshoot Circuits at the PCM

1. Pull back the carpet, and remove the passenger's console lower cover.

1. Inspect the circuit on the PCM, according to the DTC troubleshooting with a digital multitester (A) and tapered tip probe (B) as shown.

1. If you cannot get to the wire side of the connector or the wire side is sealed, disconnect the connector and use the tester probe to probe the connectors from the terminal side. Do not force the probe into the connector.