DTC P1298: ELD Circuit High Voltage NOTE:

- Information marked with an asterisk ( * ) applies to the 2004 model.
- Information marked with double asterisk ( ** ) applies to the 2005 model.

1. Turn the ignition switch ON (II).

1. Check the ELECTRICAL LOAD DETECTOR in the DATA LIST with the HDS.

Is 0.2 A or less indicated?

YES | - | Go to Step 3 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the ELD and the ECM.■

1. Turn the ignition switch OFF.

1. Disconnect the ELD 3P connector.

1. Turn the ignition switch ON (II).

1. Measure voltage between ELD 3P connector terminal No. 1 and body ground.

Is there battery voltage?

YES | - | Go to Step 7 .
NO | - |

- 2004 model: Repair open in the wire between No. 8 FI ECU (ECM) (20 A) fuse and the ELD, then go to Step 15 .
- 2005 model: Repair open in the wire between No. 18 IG ACG (15 A) fuse and the ELD, then go to Step 15 .

1. Turn the ignition switch OFF, and wait 30 seconds.

1. Disconnect ECM connector No. 2 (58P).