1. Check for continuity between ECM/PCM connector terminal E9 and body ground.

Is there continuity?

YES | - | Repair short in the wire between the No. 19 FUEL PUMP (15 A) fuse and the ECM/PCM (E9), or between the No. 19 FUEL PUMP (15 A) fuse and PGM-FI main relay 2 (FUEL PUMP), or between the No. 19 FUEL PUMP (15 A) fuse and the immobilizer control unit. Also replace the No. 19 FUEL PUMP (15 A) fuse.■
NO | - | Go to Step 38 .

1. Remove the trunk floor trim panel.

1. Remove the access panel from the floor.

1. Disconnect the fuel pump 5P connector.