For some models: SRS components are located in this area. Review the SRS component locations LHD, SRS component location RHD and the precautions and procedures before performing repairs or service. NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.
- When prying components, use the handy remover set or equivalent.
- Apply multipurpose grease to the moving portion of the seat track.
- To prevent wrinkles in the seat cushion cover, stretch the material evenly over the pad before securing the clips, hooks, and hook strips.