NOTE: If replacement is required, always replace the synchro sleeve and hub as a set.

1. Support the bearing inner race with an appropriate sized socket (A), and push down on the mainshaft (B).

1. Measure the clearance between 2nd (C) and 3rd (D) gears with a feeler gauge (E).
   - If the clearance is more than the service limit, go to Step 3 .
   - If the clearance is within the service limit, go to Step 4 .

   Standard: | 0.06−0.19 mm (0.002−0.007 in.)
   Service Limit: | 0.3 mm (0.01 in.)