Crankshaft Pulley Removal and Installation

Special Tools Required Handle 07JAB-001020B Pulley holder attachment, HEX 50 mm 07JAB-0010400
Socket wrench, 19 mm
07JAA-001020A
Removal

1. Remove the right front tyre/wheel.

1. Remove the splash shield.

1. Hold the pulley with handle (A) and holder attachment (B).

1. Remove the bolt with a 19 mm socket (C) and breaker bar.

Installation

1. Clean the crankshaft pulley (A), crankshaft (B), bolt (C), and washer (D). Lubricate the new engine oil as shown.

1. Install the crankshaft pulley, and hold the pulley with handle (A) and holder attachment (B).

1. Tighten the bolt to 29 N·m (3.0 kgf·m, 22 lbf·ft) with a torque wrench and 19 mm socket (C). Do not use an impact wrench. If you are using a new pulley bolt or new crankshaft, tighten the bolt to 34 N·m (3.5 kgf·m, 25 lbf·ft).

1. Tighten the pulley bolt an additional 90 °.

1. Install the splash shield.

1. Install the right front tyre/wheel.