SRS components are located in this area. Review the SRS component locations LHD, RHD, and the precautions and procedures, before performing repairs or service. NOTE: LHD type is shown, RHD type is symmetrical.

1. Make sure you have the anti-theft codes for the radio and the navigation system, then write down the frequencies for the radio's preset buttons.

1. Disconnect the negative cable from the battery.

1. With air conditioning; disconnect the suction and receiver lines from the evaporator core.

1. From under the hood, open the cable clamp (A), then disconnect the heater valve cable (B) from the heater valve arm (C). Turn the heater valve arm to the fully opened position as shown.

1. When the engine is cool, drain the engine coolant from the radiator.