Cross Section of Body and Sealants - General Safety Precautions

NOTE: Follow the sealer manufactur's instuctions and apply the sealer. Make note of the following items:

- Clean the areas to be sealed with wax and grease remover.

- Wipe off any excess spot sealer with thinner. After the primer is sprayed, sealer will fill to the area where spot sealer was siped off.

- Make sure you can see the sealant when the sealed part is in its proper location. Refer to front floor, rear floor, and roof panel, rear side outer panel, and rear panel, under floor, and rear wheelhouse for the items not shown in this manual.

- When appling sealant to the engine compartment, the door opening, and the hatch gutter, try to match the appearance of the factory sealer. Wipe off any excess sealer.

- Apply sealer on any area where replacement part will cover. Smooth the sealer with a brush if necessary.