Engine Mount Positioning

1. Remove the air cleaner housing.

1. Remove the ground cable (A), then remove the upper torque rod (B).

1. Loosen the side engine mount bracket bolt (A).

1. Loosen the side engine mount bracket bolts/nut (B).

1. Loosen the transmission upper mount bracket bolt (A).

1. Loosen the transmission upper mount bolt/nuts (B).

1. Raise the vehicle on the hoist to full height.

1. Loosen the lower torque rod bolt (A).

1. Lower the vehicle on the hoist.

1. Tighten the side engine mount mounting bolts/nut in the numbered sequence shown.

1. Tighten the transmission upper mount/bracket mounting bolts/nuts in the numbered sequence shown.

1. Raise the vehicle on the hoist to full height.

1. Tighten the lower torque rod mounting bolt.

1. Lower the vehicle on the hoist.

1. Install the upper torque rod (A), then tighten the new bolts in the numbered sequence shown.

1. Install the ground cable (B).

1. Install the air cleaner housing.