Maintenance Schedule for Normal and Severe Conditions - Except EU
20,000km(1year)

This Maintenance Schedule outlines the minimum required maintenance that you should perform to ensure the trouble-free operation of vehicle. Due to regional and climatic difference, some additional service may be required. Please consult the warranty booklet for a more detailed description.
The following items must be used for ‘‘severe conditions'' indicated on schedule, if the vehicle is driven MAINLY under the specified conditions A to E.

- Engine oil and engine oil filter: A/B/C/D/E
- Transmission fluid: B/D

A: Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
B: Driving in extremely hot over 35 °C (95 °F) conditions.
C: Extensive idling, or long periods of stop-and-go driving.
D: Trailer towing, driving with a loaded roof rack, or driving in mountainous conditions.
E: Driving on muddy, dusty, or de-iced roads.

Service at the indicated distance or time whichever comes first

| Replace engine oil filter

| Check parking brake adjustment

Check the parking brake operation.

| Replace dust and pollen filter

| Check expiry date for temporary repair kit bottle (if equipped)

Visually inspect the following items:

|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks.
|  | Check tightness of screws, nuts, and joints. If necessary, retighten.

| Brake hoses and lines (including ABS lines)

Check master cylinder and ABS modulator control-unit and leakage.

| All fluid level and check for leak

Check levels and check for leaks. If necessary, add.

|  | Engine coolant
|  | MTF
|  | ATF
|  | Clutch fluid
|  | Power steering fluid
|  | Brake fluid
|  | Windshield fluid

| Exhaust system

K20Z2
K24A3
Check the exhaust pipe and muffler for damage, leaks, and tightness.

| Fuel lines and connections

|  | Check fuel lines for loose connections, cracks, and deterioration.
|  | Retighten loose connections and replace any damage parts.

Every 10,000 km (6,250 miles) or 1 year

| Replace engine oil

Every 5,000 km (3,125 miles) or 6 months

| Replace engine oil

Every 10,000 km (6,250 miles) or 6 months

| Replace engine oil filter

| Check front and rear brakes

|  | Check the brake pad and disc thickness. Check for damage or cracks.
|  | Check the calipers for damage, leaks, and tightness.

Visually inspect the following items:

| Tie-rod ends, steering gearbox, and boots

Check rack grease and steering linkage. Check the boot for damage and leaking grease.

| Suspension components

Front suspension
Rear suspension

|  | Check the bolts for tightness.
|  | Check all dust cover for deterioration and damage.

| Driveshaft boots

|  | Check the boot and boot band for cracks.
|  | Check rack grease.

Every 20,000 km (12,500 miles)

| Replace air cleaner element

Every 40,000 km (25,500 miles)

| Inspect valve clearance

Check valve clearance

Every 40,000 km (25,000 miles)

| Replace spark plugs

K20Z2
K24A3

Every 100,000 km (62,500 miles)

| Replace spark plugs

K20Z2
K24A3

At 200,000 km (125,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years

| Replace engine coolant

Use genuine Honda All Season Antifreeze/Coolant Type 2.

Every 3 years

| Replace brake fluid

|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
|  | Check that brake fluid level is between upper and lower marks on the reservoir.

Every 10,000 km (6,250 miles)

| Rotate tyres

Check tyre inflation at least once per month.