Special Tools Required Compression gauge attachment A 070AJ-RBD0110 Compression gauge attachment B 070AJ-RBD0120

1. Warm up the engine to normal operating temperature (cooling fan comes on).

1. Turn the ignition switch OFF.

1. Connect the HDS to the data link connector (DLC).

1. Select PGM-FI, INSPECTION, then ALL INJECTORS OFF function on the HDS.

1. Remove the four glow plugs.

1. Attach the compression gauge to the glow plug hole.

1. Crank the engine with the starter motor and measure the compression.

   Compression Pressure:
   Above 2.4 MPa (24.5 kgf/cm 2 , 348 psi)

1. Measure the compression on the remaining cylinders.

   Maximum Variation:
   Within 200 kPa (2.0 kgf/cm 2 , 28 psi)

1. If the compression is not within specifications, check the following items, then remeasure the compression.
   - Damaged or worn valves and seats
   - Damaged cylinder head gasket
   - Damaged or worn piston rings
   - Damaged or worn piston and cylinder bore

1. Select ECM reset to cancel the ALL INJECTORS OFF function on the HDS.