1. Mark the cam position of the adjusting bolt (A) and frame.

1. Remove the self-locking nut (B) and the adjust cam (C) while holding the adjusting bolt.

1. Install the lower arm B in the reverse order of removal, and note these items:
   - Align the cam positions of the adjusting bolt and adjusting cam with the marked positions when tightening.
   - Use a new self-locking nut on reassembly.
   - Tighten all mounting hardware to the specified torque values.
   - First install all the components and lightly tighten the bolts and nuts, then raise the suspension to load it with the vehicle's weight before fully tightening to the specified torque values.
   - Before installing the wheel, clean the mating surfaces of the brake disc/drum and the inside of the wheel.
   - Check the wheel alignment, and adjust it if necessary.