LKAS Control Unit DTC 26: LKAS Camera Malfunction

1. Clear the DTC using the HDS.

1. Turn the ignition switch OFF, then turn it ON (II).

1. Watch the adaptive cruise control (ACC)/LKAS indicator.

Does the adaptive cruise control (ACC)/LKAS indicator come on?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Check for LKAS control unit DTCs with HDS.

Is DTC 26 indicated?

YES | - | Do the troubleshoot indicated for the LKAS camera DTCs. ■
NO | - | Troubleshoot the indicated DTC.■