Exploded View 5-speed model: 6-speed model: Special Tools Required Driver, 40 mm I.D.
07746-0030100
Attachment, 30 mm I.D.
07746-0030300
NOTE:

- Refer to the Exploded View as needed during this procedure.
- 6-speed model is shown, 5-speed model similar.

1. Clean all the parts in solvent, dry them, and apply lubricant to all contact surfaces except the 3rd/4th and 5th/6th synchro hubs.

1. Install the needle bearing and 3rd gear on the mainshaft.

1. Install the double cone synchro assembly (A) by aligning the synchro cone fingers (B) with the holes in 3rd gear (C), then install the synchro spring (D).