NOTE:

- The tyre inflator is employed for the spare-tyreless models instead of a spare tyre.
- The fluid sealant used to reinflate a flat tyre must be extracted and retrieved from the inside. The out-of-date inflator and the extracted fluid sealant must be retrieved by the transactor for the sake of the environment after separated as well as oil waste such as the oil and fluid, because they include the ethylene glycol, the industrial waste. (The address and telephone number of the transactor is labeled on the bottle.)
- Replace the valve with a new one if you reuse the tyre.

Do not dispose the tyre with the fluid sealant filled.

1. Raise the vehicle, and support it with safety stands in the proper locations.

1. Deflate the tyre.

1. Cut off the valve (A) at its base, and push the remaining rubber portion of the valve into the tyre.
   Avoid damage to the wheel disk when using the tools.

1. Put the tyre on the working table, and set it up.
   NOTE: Be careful not to spill the fluid sealant from the drain hole (B).