1. A/T model: Install the shift cable (A).

1. A/T model: Install the shift cable cover (B), then tighten the shift cable holder (C).

1. Install a new set ring on the end of each driveshaft, then install the driveshafts. Make sure each ring ‘‘clicks'' into place in the differential and intermediate shaft.

1. Connect the suspension lower arm ball joints.

1. Install the damper fork.

1. Connect the stabilizer links.