NOTE: Take care not to scratch the body.

1. Remove the rear inner fender (A).

   -1. | Remove the bolt (B) from the wheel arch.
   -2. | On the front of the wheel arch, remove the screws (C) securing the side sill panel (D) and rear inner fender.
   -3. | On the rear bumper (E), remove the screws (C, F).
   -4. | From the wheel arch, remove the clips (G, H, I).
   -5. | Pull the rear inner fender out.

1. Install the inner fender in the reverse order of removal, and note these items:
   - Replace any damaged clips.
   - Push the clips into place securely.