Special Tools Required Stem seal driver 07PAD-0010000 Valve spring compressor attachment 07757-PJ10100
Valve spring compressor
07757-0010000

1. Coat the valve stems with engine oil. Install the valves in the valve guides.

1. Check that the valves move up and down smoothly.

1. Install the spring seats on the cylinder head.

1. Install the new valve seals (A) using the valve guide seal installer (B).
   NOTE: The exhaust valve seal (C) has a black spring (D), and the intake valve seal (E) has a white spring (F). They are not interchangeable.

1. Install the valve springs. Place the end of the valve spring with closely wound coils toward the cylinder head.

1. Install the valve retainer.