Maintenance Schedule for Severe Conditions - EU
200,000km(10year)

Follow the Severe Conditions Maintenance Schedule if the customer's vehicle is driven MAINLY under one or more of the following conditions:

- Driving less than 8 km (5 miles) per trip or, in freezing temperatures, driving less than 16 km (10 miles) per trip.
- Driving in extremely hot over 35 °C (95 °F) conditions.
- Extensive idling, or long periods of stop-and-go driving.
- Trailer towing, driving with a car-top carrier, or driving in mountainous conditions.
- Driving on muddy, dusty, or de-iced roads.

NOTE: If the vehicle is driven OCCASIONALLY under severe conditions, follow the Normal Conditions Maintenance Schedule.

Service at the indicated distance or time whichever comes first

| Replace engine oil filter

| Inspect drive belt

Look for cracks and damage, then check the position of the drive belt auto-tensioner indicator.

| Check parking brake adjustment

Check the parking brake operation.

| Replace dust and pollen filter

When the vehicle is driven primarily in urban areas that have high concentrations of soot in the air, under dusty conditions of the air flow from the heating and air conditioning system becomes less than normal.

| Check lights alignment

Check the position of the headlights.

| Test drive (noise, stability, dashboard operation)

| Check expiry date for temporary repair kit bottle (if equipped)

Visually inspect the following items:

|  | Check for correct installation and position, check for cracks, deterioration, rust, and leaks.
|  | Check tightness of screws, nuts, and joints. If necessary, retighten.

| Brake hoses and lines (including ABS/VSA lines)

Check the master cylinder and ABS/VSA modulator- control unit and leakage.

| All fluid levels and condition of fluid

Check levels and check for leaks. If necessary, add.

|  | Engine coolant
|  | MTF
|  | ATF
|  | Clutch fluid
|  | Power steering fluid
|  | Brake fluid
|  | Windshield fluid

| Exhaust system

K20Z2 , K24A3
Check the catalytic converter heat shield, exhaust pipe, and muffler for damage, leaks, and tightness.

| Fuel lines and connections

|  | Check fuel lines for loose connections, cracks, and deterioration.
|  | Retighten loose connections and replace any damaged parts.

| Tyre condition

Every 10,000 km (6,250 miles) or 6 months

| Replace engine oil

| Check front and rear brakes

|  | Check the brake pad and disc thickness. Check for damage or cracks.
|  | Check the calipers for damage, leaks, and tightness.

Visually inspect the following items:

| Tie-rod ends, steering gearbox, and boots

|  | Check rack grease and steering linkage.
|  | Check the boot for damage and leaking grease.

| Suspension components

Front suspension
Rear suspension

|  | Check the bolts for tightness.
|  | Check all dust covers for deterioration and damage.

| Driveshaft boots

|  | Check the boot and boot band for cracks.
|  | Check rack grease.

Every 20,000 km (12,500 miles)

| Replace air cleaner element

Use normal conditions except in dusty conditions.

Every 40,000 km (25,000 miles)

| Inspect valve clearance

| Replace spark plugs

K20Z2
K24A3

Every 120,000 km (75,000 miles)

| Replace spark plugs

K20Z2
K24A3

At 200,000 km (120,000 miles) or 10 years, then every 100,000 km (60,000 miles) or 5 years

| Replace engine coolant

Use genuine Honda All Season Antifreeze/Coolant Type 2.

Every 60,000 km (37,500 miles) or 4 years

| Replace Manual Transmission Fluid (MTF)

Use genuine Honda MTF.

At 60,000 km (37,500 miles) or 4 years, then every 40,000 km (25,000 miles) or 2 years

| Replace Automatic Transmission Fluid (ATF)

Use genuine Honda ATF-Z1.
K20Z2
K24A3

Every 3 years

| Replace brake fluid

|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
|  | Check the brake fluid level is between the upper and lower marks on the reservoir.

Every year

| Inspect vehicle corrosion:

refer to the Body Repair Manual

|  | External paintwork and panel corrosion check
|  | Under body corrosion check