How to Remove the ECM/PCM for Testing If DTC troubleshooting requires voltage or resistance checks at the ECM/PCM connectors, remove the ECM/PCM and test it:

1. Jump the SCS line with the HDS.

1. Remove the center lower covers (A).

1. Remove the duct (B).

1. Disconnect the ECM/PCM connectors (C).

1. Remove the bolts (D), then remove the ECM/PCM (E).

1. Install the ECM/PCM in the reverse order of removal.

1. Open the SCS line with the HDS.