Pulser Test

1. Reconnect the 6P connector to the window motor.

1. Check for voltage between the terminals.
   - There should be battery voltage between the No. 6 [No. 1] (+) and No. 5 [No. 2] (−) terminals when the ignition switch is ON (II).
   - Connect an analog voltmeter between the No. 2 [No. 5] (+) and No. 5 [No. 2] (−) terminals, and run the window motor down or up. The voltmeter needle should move back and forth alternately (a digital voltmeter should show the average voltage between 0−5 V).
   - Connect an analog voltmeter between the No. 3 [No. 4] (+) and No. 5 [No. 2] (−) terminals, and run the window motor down or up. The voltmeter needle should move back and forth alternately.
     If it does not, replace the driver's window motor.
   [ ]: RHD type